Record of tests for thermocouple sensor

June 22, 2019

* Had some troubles with MAX6675 library and code, used the sample code given with the library and worked
* Tested the thermocouple by dipping into kettle boiled tap water
* Max temperature recorded: 98⁰ C