Record of tests for thermocouple sensor

June 22, 2019

* Had some troubles with MAX6675 library and code, used the sample code given with the library and worked
* Tested the thermocouple by dipping into kettle boiled tap water
* Max temperature recorded: 98⁰ C

June 29, 2019

* Calibrated thermocouples with ice water (0⁰ C)
* Used breadboard to consolidate clock for serial read of thermocouples
* Waited for temperature readings to settle before recording temperature offsets